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P2.5 led display details information 
Product: P2.5 indoor full color          
Module size: 160*160mm      
Pixel density: 160000 dots/m²          
LED lamp: SMD2121
Module resolution: 64*64
Module consumption: 30W/piece  
Viewing distance: 3-15m   
Max power consumption: 1200W/m²     
Standard cabinet size: 480*480mm   
Drive mode: 1/32 scan
Brightness: 1200-1500cd/m²   
Hub mode: hub75
Drive IC: MBI5124  
Frame frequency: ≧60Hz/s    
Refresh rate: 360-1920Hz/s 
 MTTF: >5000 hours  
Life time: >100,000 hours  
Defect rate: <0.0001  
Video signal input: RF, S-video, RGB, RGBHV, YUV, YC, composition
Temperature range:Storage: -20 to 65°C
Working: -20 to 50°C    
Gray scale/color: 4096 grades for R ,G and B      
Display:  ≥16.7m colors  
Working voltage: 110/220V AC
Viewing angle:
Horizontal: 120º  
Vertical: 120º  
Display content: videos, pictures and graphics
Operating humidity: 10-90%  
 Storage humidity: 10-90%   
Continue working time: 24 hours  
Controlmode:synchronization   
[bookmark: _GoBack]Module price:18.68USD/PCS(with tax rate price)
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